

|  |
| --- |
| **SYSTEM : DURABLE HEAVY TEXTURE - WMC FOR EXTERIORS** |
| **Concrete and Masonry Surface – Exterior** |

**System Description**

**Primary Coat: 1 coat Weathercoat AR Primer**

A premium quality acrylic co-polymer based primer with good alkali resisting properties designed to provide a sound base for texture coating from the Berger range.

**Volume Solids:** 40% ± 2%

**Top Coat: 2 coats of Select Heavy Texture (WMC)**

A heavy texture coating based on a tough, flexible acrylic co-polymer resin, pigmented with titanium dioxide and other light fast pigments reinforced with selected mineral quartz, mica and marble chips. Its formulation incorporating fungicides and algaecides, and its heavy build ensures good weather resistance, and also helps cover hairline surface cracks and irregularities.helps cover hairline surface cracks and irregularities.

**Volume Solids:** 68% ± 2%

**Recommended Areas of Application**

**Area of Use:** Exterior & Interior

**Substrate:** Concrete, Plaster, Masonry, Brickwork, Block work, Timber.

