

|  |
| --- |
| **SYSTEM : PREMIUM FINISH FOR WOOD - INTERIOR (CLEAR)** |
| **Wood - Interior (Clear)** |

**Primary Coat: 2-3 coats of Touchwood PU sanding sealer interior**

Based on acrylic resin isocyanate and has excellent grain filling properties.

**Volume Solids: 46% ± 2%**

**VOC: <275 gms/ltr complies to LEED Standard**

**Top Coats: 1-2 coats of Touchwood PU Topcoat (Clear)**

A two pack polyurethane coating based on suitably modified polyester containing special additives to provide a smooth, tough, durable and hardwearing low sheen finish with good flow and film build-up.

Highlights:

a) Excellent leveling and very fast drying

b) Gloss/Silk Matt/Matt Finish with good hardness

c) Good resistance to household chemicals and beverages

**Volume Solids:** 47% ± 2%

**Recommended Areas of Application**

**Area of Use:** Interior only

**Substrate:** Wood and related substrates

****